The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> mbrlen - get number of bytes in a character (restartable)

#### SYNOPSIS

> ``#include <wchar.h>
> size_t mbrlen(const char *restrict` s`, size_t` n`,
> mbstate_t *restrict` ps`);
> ``

#### DESCRIPTION

> [CX] The functionality described on this reference page is aligned with the ISO C standard. Any conflict between the requirements described here and the ISO C standard is unintentional. This volume of IEEE Std 1003.1-2001 defers to the ISO C standard.

> If s is not a null pointer, mbrlen() shall determine the number of bytes constituting the character pointed to by s. It shall be equivalent to:

>     mbstate_t internal;
>     mbrtowc(NULL, s, n, ps != NULL ? ps : &internal);

> If ps is a null pointer, the mbrlen() function shall use its own internal mbstate_t object, which is initialized at program start-up to the initial conversion state. Otherwise, the mbstate_t object pointed to by ps shall be used to completely describe the current conversion state of the associated character sequence. The implementation shall behave as if no function defined in this volume of IEEE Std 1003.1-2001 calls mbrlen().

> The behavior of this function is affected by the LC_CTYPE category of the current locale.

#### RETURN VALUE

> The mbrlen() function shall return the first of the following that applies:

> 0
>   If the next n or fewer bytes complete the character that corresponds to the null wide character.
> positive
>   If the next n or fewer bytes complete a valid character; the value returned shall be the number of bytes that complete the character.
> (size_t)-2
>   If the next n bytes contribute to an incomplete but potentially valid character, and all n bytes have been processed. When n has at least the value of the {MB_CUR_MAX} macro, this case can only occur if s points at a sequence of redundant shift sequences (for implementations with state-dependent encodings).
> (size_t)-1
>   If an encoding error occurs, in which case the next n or fewer bytes do not contribute to a complete and valid character. In this case, [EILSEQ] shall be stored in errno and the conversion state is undefined.

#### ERRORS

> The mbrlen() function may fail if:

> [EINVAL]
>   ps points to an object that contains an invalid conversion state.
> [EILSEQ]
>   Invalid character sequence is detected.

The following sections are informative.

#### EXAMPLES

> None.

#### APPLICATION USAGE

> None.

#### RATIONALE

> None.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> mbsinit(), mbrtowc(), the Base Definitions volume of IEEE Std 1003.1-2001, <wchar.h>

#### CHANGE HISTORY

> First released in Issue 5. Included for alignment with ISO/IEC 9899:1990/Amendment 1:1995 (E).

#### Issue 6

> The mbrlen() prototype is updated for alignment with the ISO/IEC 9899:1999 standard.

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]