The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> sockatmark - determine whether a socket is at the out-of-band mark

#### SYNOPSIS

> ``#include <sys/socket.h>
> int sockatmark(int` s`);
> ``

#### DESCRIPTION

> The sockatmark() function shall determine whether the socket specified by the descriptor s is at the out-of-band data mark (see the System Interfaces volume of IEEE Std 1003.1-2001, Section 2.10.12, Socket Out-of-Band State). If the protocol for the socket supports out-of-band data by marking the stream with an out-of-band data mark, the sockatmark() function shall return 1 when all data preceding the mark has been read and the out-of-band data mark is the first element in the receive queue. The sockatmark() function shall not remove the mark from the stream.

#### RETURN VALUE

> Upon successful completion, the sockatmark() function shall return a value indicating whether the socket is at an out-of-band data mark. If the protocol has marked the data stream and all data preceding the mark has been read, the return value shall be 1; if there is no mark, or if data precedes the mark in the receive queue, the sockatmark() function shall return 0. Otherwise, it shall return a value of -1 and set errno to indicate the error.

#### ERRORS

> The sockatmark() function shall fail if:

> [EBADF]
>   The s argument is not a valid file descriptor.
> [ENOTTY]
>   The s argument does not specify a descriptor for a socket.

The following sections are informative.

#### EXAMPLES

> None.

#### APPLICATION USAGE

> The use of this function between receive operations allows an application to determine which received data precedes the out-of-band data and which follows the out-of-band data.

> There is an inherent race condition in the use of this function. On an empty receive queue, the current read of the location might well be at the "mark", but the system has no way of knowing that the next data segment that will arrive from the network will carry the mark, and sockatmark() will return false, and the next read operation will silently consume the mark.

> Hence, this function can only be used reliably when the application already knows that the out-of-band data has been seen by the system or that it is known that there is data waiting to be read at the socket (via SIGURG or select()). See Socket Receive Queue , Socket Out-of-Band Data State , Signals , and pselect() for details.

#### RATIONALE

> The sockatmark() function replaces the historical SIOCATMARK command to ioctl() which implemented the same functionality on many implementations. Using a wrapper function follows the adopted conventions to avoid specifying commands to the ioctl() function, other than those now included to support XSI STREAMS. The sockatmark() function could be implemented as follows:

>     #include <sys/ioctl.h>

>     int sockatmark(int s)
>     {
>         int val;
>         if (ioctl(s,SIOCATMARK,&val)==-1)
>             return(-1);
>         return(val);
>     }

> The use of [ENOTTY] to indicate an incorrect descriptor type matches the historical behavior of SIOCATMARK.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> pselect(), recv(), recvmsg(), the Base Definitions volume of IEEE Std 1003.1-2001, <sys/socket.h>

#### CHANGE HISTORY

> First released in Issue 6. Derived from IEEE Std 1003.1g-2000.

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]