The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> tcsetattr - set the parameters associated with the terminal

#### SYNOPSIS

> ``#include <termios.h>
> int tcsetattr(int` fildes`, int` optional_actions`,
> const struct termios *`termios_p`);
> ``

#### DESCRIPTION

> The tcsetattr() function shall set the parameters associated with the terminal referred to by the open file descriptor fildes (an open file descriptor associated with a terminal) from the termios structure referenced by termios_p as follows:

> - If optional_actions is TCSANOW, the change shall occur immediately.

> - If optional_actions is TCSADRAIN, the change shall occur after all output written to fildes is transmitted. This function should be used when changing parameters that affect output.

> - If optional_actions is TCSAFLUSH, the change shall occur after all output written to fildes is transmitted, and all input so far received but not read shall be discarded before the change is made.

> If the output baud rate stored in the termios structure pointed to by termios_p is the zero baud rate, B0, the modem control lines shall no longer be asserted. Normally, this shall disconnect the line.

> If the input baud rate stored in the termios structure pointed to by termios_p is 0, the input baud rate given to the hardware is the same as the output baud rate stored in the termios structure.

> The tcsetattr() function shall return successfully if it was able to perform any of the requested actions, even if some of the requested actions could not be performed. It shall set all the attributes that the implementation supports as requested and leave all the attributes not supported by the implementation unchanged. If no part of the request can be honored, it shall return -1 and set errno to [EINVAL]. If the input and output baud rates differ and are a combination that is not supported, neither baud rate shall be changed. A subsequent call to tcgetattr() shall return the actual state of the terminal device (reflecting both the changes made and not made in the previous tcsetattr() call). The tcsetattr() function shall not change the values found in the termios structure under any circumstances.

> The effect of tcsetattr() is undefined if the value of the termios structure pointed to by termios_p was not derived from the result of a call to tcgetattr() on fildes; an application should modify only fields and flags defined by this volume of IEEE Std 1003.1-2001 between the call to tcgetattr() and tcsetattr(), leaving all other fields and flags unmodified.

> No actions defined by this volume of IEEE Std 1003.1-2001, other than a call to tcsetattr() or a close of the last file descriptor in the system associated with this terminal device, shall cause any of the terminal attributes defined by this volume of IEEE Std 1003.1-2001 to change.

> If tcsetattr() is called from a process which is a member of a background process group on a fildes associated with its controlling terminal:

> - If the calling process is blocking or ignoring SIGTTOU signals, the operation completes normally and no signal is sent.

> - Otherwise, a SIGTTOU signal shall be sent to the process group.

#### RETURN VALUE

> Upon successful completion, 0 shall be returned. Otherwise, -1 shall be returned and errno set to indicate the error.

#### ERRORS

> The tcsetattr() function shall fail if:

> [EBADF]
>   The fildes argument is not a valid file descriptor.
> [EINTR]
>   A signal interrupted tcsetattr().
> [EINVAL]
>   The optional_actions argument is not a supported value, or an attempt was made to change an attribute represented in the termios structure to an unsupported value.
> [ENOTTY]
>   The file associated with fildes is not a terminal.

> The tcsetattr() function may fail if:

> [EIO]
>   The process group of the writing process is orphaned, and the writing process is not ignoring or blocking SIGTTOU.

The following sections are informative.

#### EXAMPLES

> None.

#### APPLICATION USAGE

> If trying to change baud rates, applications should call tcsetattr() then call tcgetattr() in order to determine what baud rates were actually selected.

#### RATIONALE

> The tcsetattr() function can be interrupted in the following situations:

> - It is interrupted while waiting for output to drain.

> - It is called from a process in a background process group and SIGTTOU is caught.

> See also the RATIONALE section in tcgetattr().

#### FUTURE DIRECTIONS

> Using an input baud rate of 0 to set the input rate equal to the output rate may not necessarily be supported in a future version of this volume of IEEE Std 1003.1-2001.

#### SEE ALSO

> cfgetispeed(), tcgetattr(), the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface, <termios.h>, <unistd.h>

#### CHANGE HISTORY

> First released in Issue 3. Included for alignment with the POSIX.1-1988 standard.

#### Issue 6

> The following new requirements on POSIX implementations derive from alignment with the Single UNIX Specification:

> - In the DESCRIPTION, text previously conditional on _POSIX_JOB_CONTROL is now mandated. This is a FIPS requirement.

> - The [EIO] error is added.

> In the DESCRIPTION, the text describing use of tcsetattr() from a process which is a member of a background process group is clarified.

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]