The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> posix_trace_get_attr, posix_trace_get_status - retrieve the trace attributes or trace status (TRACING)

#### SYNOPSIS

> ``[TRC] #include <trace.h>
> int posix_trace_get_attr(trace_id_t` trid`, trace_attr_t *`attr`);
> int posix_trace_get_status(trace_id_t` trid`,
> struct posix_trace_status_info *`statusinfo`);``
> `
> `

#### DESCRIPTION

> The posix_trace_get_attr() function shall copy the attributes of the active trace stream identified by trid into the object pointed to by the attr argument. [TRL] If the Trace Log option is supported, trid may represent a pre-recorded trace log.

> The posix_trace_get_status() function shall return, in the structure pointed to by the statusinfo argument, the current trace status for the trace stream identified by the trid argument. These status values returned in the structure pointed to by statusinfo shall have been appropriately read to ensure that the returned values are consistent. [TRL] If the Trace Log option is supported and the trid argument refers to a pre-recorded trace stream, the status shall be the status of the completed trace stream.

> Each time the posix_trace_get_status() function is used, the overrun status of the trace stream shall be reset to POSIX_TRACE_NO_OVERRUN immediately after the call completes. [TRL] If the Trace Log option is supported, the posix_trace_get_status() function shall behave the same as when the option is not supported except for the following differences:

> - If the trid argument refers to a trace stream with log, each time the posix_trace_get_status() function is used, the log overrun status of the trace stream shall be reset to POSIX_TRACE_NO_OVERRUN and the flush_error status shall be reset to zero immediately after the call completes.

> - If the trid argument refers to a pre-recorded trace stream, the status returned shall be the status of the completed trace stream and the status values of the trace stream shall not be reset.

#### RETURN VALUE

> Upon successful completion, these functions shall return a value of zero. Otherwise, they shall return the corresponding error number.

> The posix_trace_get_attr() function stores the trace attributes in the object pointed to by attr, if successful.

> The posix_trace_get_status() function stores the trace status in the object pointed to by statusinfo, if successful.

#### ERRORS

> These functions shall fail if:

> [EINVAL]
>   The trace stream argument trid does not correspond to a valid active trace stream or a valid trace log.

The following sections are informative.

#### EXAMPLES

> None.

#### APPLICATION USAGE

> None.

#### RATIONALE

> None.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> posix_trace_attr_destroy(), posix_trace_attr_init(), posix_trace_create() , posix_trace_open(), the Base Definitions volume of IEEE Std 1003.1-2001, <trace.h>

#### CHANGE HISTORY

> First released in Issue 6. Derived from IEEE Std 1003.1q-2000.

> IEEE PASC Interpretation 1003.1 #123 is applied.

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]