The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> sigtimedwait, sigwaitinfo - wait for queued signals (REALTIME)

#### SYNOPSIS

> ``[RTS] #include <signal.h>
> int sigtimedwait(const sigset_t *restrict` set`,
> siginfo_t *restrict` info`,
> const struct timespec *restrict` timeout`);
> int sigwaitinfo(const sigset_t *restrict` set`,
> siginfo_t *restrict` info`);``
> `
> `

#### DESCRIPTION

> The sigtimedwait() function shall be equivalent to sigwaitinfo() except that if none of the signals specified by set are pending, sigtimedwait() shall wait for the time interval specified in the timespec structure referenced by timeout. If the timespec structure pointed to by timeout is zero-valued and if none of the signals specified by set are pending, then sigtimedwait() shall return immediately with an error. If timeout is the NULL pointer, the behavior is unspecified. [MON] If the Monotonic Clock option is supported, the CLOCK_MONOTONIC clock shall be used to measure the time interval specified by the timeout argument.

> The sigwaitinfo() function selects the pending signal from the set specified by set. Should any of multiple pending signals in the range SIGRTMIN to SIGRTMAX be selected, it shall be the lowest numbered one. The selection order between realtime and non-realtime signals, or between multiple pending non-realtime signals, is unspecified. If no signal in set is pending at the time of the call, the calling thread shall be suspended until one or more signals in set become pending or until it is interrupted by an unblocked, caught signal.

> The sigwaitinfo() function shall be equivalent to the sigwait() function if the info argument is NULL. If the info argument is non-NULL, the sigwaitinfo() function shall be equivalent to sigwait(), except that the selected signal number shall be stored in the si_signo member, and the cause of the signal shall be stored in the si_code member. If any value is queued to the selected signal, the first such queued value shall be dequeued and, if the info argument is non-NULL, the value shall be stored in the si_value member of info. The system resource used to queue the signal shall be released and returned to the system for other use. If no value is queued, the content of the si_value member is undefined. If no further signals are queued for the selected signal, the pending indication for that signal shall be reset.

#### RETURN VALUE

> Upon successful completion (that is, one of the signals specified by set is pending or is generated) sigwaitinfo() and sigtimedwait() shall return the selected signal number. Otherwise, the function shall return a value of -1 and set errno to indicate the error.

#### ERRORS

> The sigtimedwait() function shall fail if:

> [EAGAIN]
>   No signal specified by set was generated within the specified timeout period.

> The sigtimedwait() and sigwaitinfo() functions may fail if:

> [EINTR]
>   The wait was interrupted by an unblocked, caught signal. It shall be documented in system documentation whether this error causes these functions to fail.

> The sigtimedwait() function may also fail if:

> [EINVAL]
>   The timeout argument specified a tv_nsec value less than zero or greater than or equal to 1000 million.

> An implementation should only check for this error if no signal is pending in set and it is necessary to wait.

The following sections are informative.

#### EXAMPLES

> None.

#### APPLICATION USAGE

> The sigtimedwait() function times out and returns an [EAGAIN] error. Application writers should note that this is inconsistent with other functions such as pthread_cond_timedwait() that return [ETIMEDOUT].

#### RATIONALE

> Existing programming practice on realtime systems uses the ability to pause waiting for a selected set of events and handle the first event that occurs in-line instead of in a signal-handling function. This allows applications to be written in an event-directed style similar to a state machine. This style of programming is useful for largescale transaction processing in which the overall throughput of an application and the ability to clearly track states are more important than the ability to minimize the response time of individual event handling.

> It is possible to construct a signal-waiting macro function out of the realtime signal function mechanism defined in this volume of IEEE Std 1003.1-2001. However, such a macro has to include the definition of a generalized handler for all signals to be waited on. A significant portion of the overhead of handler processing can be avoided if the signal-waiting function is provided by the kernel. This volume of IEEE Std 1003.1-2001 therefore provides two signal-waiting functions-one that waits indefinitely and one with a timeout-as part of the overall realtime signal function specification.

> The specification of a function with a timeout allows an application to be written that can be broken out of a wait after a set period of time if no event has occurred. It was argued that setting a timer event before the wait and recognizing the timer event in the wait would also implement the same functionality, but at a lower performance level. Because of the performance degradation associated with the user-level specification of a timer event and the subsequent cancellation of that timer event after the wait completes for a valid event, and the complexity associated with handling potential race conditions associated with the user-level method, the separate function has been included.

> Note that the semantics of the sigwaitinfo() function are nearly identical to that of the sigwait() function defined by this volume of IEEE Std 1003.1-2001. The only difference is that sigwaitinfo() returns the queued signal value in the value argument. The return of the queued value is required so that applications can differentiate between multiple events queued to the same signal number.

> The two distinct functions are being maintained because some implementations may choose to implement the POSIX Threads Extension functions and not implement the queued signals extensions. Note, though, that sigwaitinfo() does not return the queued value if the value argument is NULL, so the POSIX Threads Extension sigwait() function can be implemented as a macro on sigwaitinfo().

> The sigtimedwait() function was separated from the sigwaitinfo() function to address concerns regarding the overloading of the timeout pointer to indicate indefinite wait (no timeout), timed wait, and immediate return, and concerns regarding consistency with other functions where the conditional and timed waits were separate functions from the pure blocking function. The semantics of sigtimedwait() are specified such that sigwaitinfo() could be implemented as a macro with a NULL pointer for timeout.

> The sigwait functions provide a synchronous mechanism for threads to wait for asynchronously-generated signals. One important question was how many threads that are suspended in a call to a sigwait() function for a signal should return from the call when the signal is sent. Four choices were considered:

> 1. Return an error for multiple simultaneous calls to sigwait functions for the same signal.

> 2. One or more threads return.

> 3. All waiting threads return.

> 4. Exactly one thread returns.

> Prohibiting multiple calls to sigwait() for the same signal was felt to be overly restrictive. The "one or more" behavior made implementation of conforming packages easy at the expense of forcing POSIX threads clients to protect against multiple simultaneous calls to sigwait() in application code in order to achieve predictable behavior. There was concern that the "all waiting threads" behavior would result in "signal broadcast storms", consuming excessive CPU resources by replicating the signals in the general case. Furthermore, no convincing examples could be presented that delivery to all was either simpler or more powerful than delivery to one.

> Thus, the consensus was that exactly one thread that was suspended in a call to a sigwait function for a signal should return when that signal occurs. This is not an onerous restriction as:

> - A multi-way signal wait can be built from the single-way wait.

> - Signals should only be handled by application-level code, as library routines cannot guess what the application wants to do with signals generated for the entire process.

> - Applications can thus arrange for a single thread to wait for any given signal and call any needed routines upon its arrival.

> In an application that is using signals for interprocess communication, signal processing is typically done in one place. Alternatively, if the signal is being caught so that process cleanup can be done, the signal handler thread can call separate process cleanup routines for each portion of the application. Since the application main line started each portion of the application, it is at the right abstraction level to tell each portion of the application to clean up.

> Certainly, there exist programming styles where it is logical to consider waiting for a single signal in multiple threads. A simple sigwait_multiple() routine can be constructed to achieve this goal. A possible implementation would be to have each sigwait_multiple() caller registered as having expressed interest in a set of signals. The caller then waits on a thread-specific condition variable. A single server thread calls a sigwait() function on the union of all registered signals. When the sigwait() function returns, the appropriate state is set and condition variables are broadcast. New sigwait_multiple() callers may cause the pending sigwait() call to be canceled and reissued in order to update the set of signals being waited for.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> Realtime Signals, pause(), pthread_sigmask(), sigaction(), sigpending(), sigsuspend(), sigwait(), the Base Definitions volume of IEEE Std 1003.1-2001, <signal.h>, <time.h>

#### CHANGE HISTORY

> First released in Issue 5. Included for alignment with the POSIX Realtime Extension and the POSIX Threads Extension.

#### Issue 6

> These functions are marked as part of the Realtime Signals Extension option.

> The Open Group Corrigendum U035/3 is applied. The SYNOPSIS of the sigwaitinfo() function has been corrected so that the second argument is of type siginfo_t *.

> The [ENOSYS] error condition has been removed as stubs need not be provided if an implementation does not support the Realtime Signals Extension option.

> The DESCRIPTION is updated for alignment with IEEE Std 1003.1j-2000 by specifying that the CLOCK_MONOTONIC clock, if supported, is used to measure timeout intervals.

> The restrict keyword is added to the sigtimedwait() and sigwaitinfo() prototypes for alignment with the ISO/IEC 9899:1999 standard.

> IEEE Std 1003.1-2001/Cor 2-2004, item XSH/TC2/D6/130 is applied, restoring wording in the RETURN VALUE section to that in the original base document (``An implementation should only check for this error if no signal is pending in set and it is necessary to wait").

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]