The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> posix_trace_eventid_equal, posix_trace_eventid_get_name, posix_trace_trid_eventid_open - manipulate the trace event type identifier (TRACING)

#### SYNOPSIS

> ``[TRC] #include <trace.h>
> int posix_trace_eventid_equal(trace_id_t` trid`, trace_event_id_t` event1`,
> trace_event_id_t` event2`);
> int posix_trace_eventid_get_name(trace_id_t` trid`,
> trace_event_id_t` event`, char *`event_name`);
> ``
> ``[TRC TEF] int posix_trace_trid_eventid_open(trace_id_t` trid`,
> const char *restrict` event_name`,
> trace_event_id_t *restrict` event`);``
> `
> `

#### DESCRIPTION

> The posix_trace_eventid_equal() function shall compare the trace event type identifiers event1 and event2 from the same trace stream or the same trace log identified by the trid argument. If the trace event type identifiers event1 and event2 are from different trace streams, the return value shall be unspecified.

> The posix_trace_eventid_get_name() function shall return, in the argument pointed to by event_name, the trace event name associated with the trace event type identifier identified by the argument event, for the trace stream or for the trace log identified by the trid argument. The name of the trace event shall have a maximum of {TRACE_EVENT_NAME_MAX} characters (which has the minimum value {_POSIX_TRACE_EVENT_NAME_MAX}). Successive calls to this function with the same trace event type identifier and the same trace stream identifier shall return the same event name.

> [TEF] The posix_trace_trid_eventid_open() function shall associate a user trace event name with a trace event type identifier for a given trace stream. The trace stream is identified by the trid argument, and it shall be an active trace stream. The trace event name is the string pointed to by the argument event_name. It shall have a maximum of {TRACE_EVENT_NAME_MAX} characters (which has the minimum value {_POSIX_TRACE_EVENT_NAME_MAX}). The number of user trace event type identifiers that can be defined for any given process is limited by the maximum value {TRACE_USER_EVENT_MAX}, which has the minimum value {_POSIX_TRACE_USER_EVENT_MAX}.

> If the Trace Inherit option is not supported, the posix_trace_trid_eventid_open() function shall associate the user trace event name pointed to by the event_name argument with a trace event type identifier that is unique for the process being traced in the trace stream identified by the trid argument, and is returned in the variable pointed to by the event argument. If the user trace event name has already been mapped for the traced process, then the previously assigned trace event type identifier shall be returned. If the per-process user trace event name limit represented by {TRACE_USER_EVENT_MAX} has been reached, the pre-defined POSIX_TRACE_UNNAMED_USEREVENT (see Trace Option: User Trace Event ) user trace event shall be returned.

> [TEF TRI] If the Trace Inherit option is supported, the posix_trace_trid_eventid_open() function shall associate the user trace event name pointed to by the event_name argument with a trace event type identifier that is unique for all the processes being traced in the trace stream identified by the trid argument, and is returned in the variable pointed to by the event argument. If the user trace event name has already been mapped for the traced processes, then the previously assigned trace event type identifier shall be returned. If the per-process user trace event name limit represented by {TRACE_USER_EVENT_MAX} has been reached, the pre-defined POSIX_TRACE_UNNAMED_USEREVENT (see Trace Option: User Trace Event ) user trace event shall be returned.

#### RETURN VALUE

> Upon successful completion, the posix_trace_eventid_get_name() and [TEF] posix_trace_trid_eventid_open() functions shall return a value of zero. Otherwise, they shall return the corresponding error number.

> The posix_trace_eventid_equal() function shall return a non-zero value if event1 and event2 are equal; otherwise, a value of zero shall be returned. No errors are defined. If either event1 or event2 are not valid trace event type identifiers for the trace stream specified by trid or if the trid is invalid, the behavior shall be unspecified.

> The posix_trace_eventid_get_name() function stores the trace event name value in the object pointed to by event_name, if successful.

> [TEF] The posix_trace_trid_eventid_open() function stores the trace event type identifier value in the object pointed to by event, if successful.

#### ERRORS

> The posix_trace_eventid_get_name() and [TEF] posix_trace_trid_eventid_open() functions shall fail if:

> [EINVAL]
>   The trid argument was not a valid trace stream identifier.

> [TEF] The posix_trace_trid_eventid_open() function shall fail if:

> [ENAMETOOLONG]
>   [TEF]
>   The size of the name pointed to by the event_name argument was longer than the implementation-defined value {TRACE_EVENT_NAME_MAX}.

> The posix_trace_eventid_get_name() function shall fail if:

> [EINVAL]
>   The trace event type identifier event was not associated with any name.

The following sections are informative.

#### EXAMPLES

> None.

#### APPLICATION USAGE

> None.

#### RATIONALE

> None.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> Trace Option: User Trace Event, posix_trace_event(), posix_trace_getnext_event(), the Base Definitions volume of IEEE Std 1003.1-2001, <trace.h>

#### CHANGE HISTORY

> First released in Issue 6. Derived from IEEE Std 1003.1q-2000.

> IEEE PASC Interpretations 1003.1 #123 and #129 are applied.

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]