The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> stty - set the options for a terminal

#### SYNOPSIS

> ``stty` [ `-a| -g`]`
> stty` operands`
> ``

#### DESCRIPTION

> The stty utility shall set or report on terminal I/O characteristics for the device that is its standard input. Without options or operands specified, it shall report the settings of certain characteristics, usually those that differ from implementation-defined defaults. Otherwise, it shall modify the terminal state according to the specified operands. Detailed information about the modes listed in the first five groups below are described in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface. Operands in the Combination Modes group (see Combination Modes) are implemented using operands in the previous groups. Some combinations of operands are mutually-exclusive on some terminal types; the results of using such combinations are unspecified.

> Typical implementations of this utility require a communications line configured to use the termios interface defined in the System Interfaces volume of IEEE Std 1003.1-2001. On systems where none of these lines are available, and on lines not currently configured to support the termios interface, some of the operands need not affect terminal characteristics.

#### OPTIONS

> The stty utility shall conform to the Base Definitions volume of IEEE Std 1003.1-2001, Section 12.2, Utility Syntax Guidelines.

> The following options shall be supported:

> -a
>   Write to standard output all the current settings for the terminal.
> -g
>   Write to standard output all the current settings in an unspecified form that can be used as arguments to another invocation of the stty utility on the same system. The form used shall not contain any characters that would require quoting to avoid word expansion by the shell; see Word Expansions.

#### OPERANDS

> The following operands shall be supported to set the terminal characteristics.

> ##### Control Modes

> parenb (-parenb)
>   Enable (disable) parity generation and detection. This shall have the effect of setting (not setting) PARENB in the termios c_cflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> parodd (-parodd)
>   Select odd (even) parity. This shall have the effect of setting (not setting) PARODD in the termios c_cflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> cs5 cs6 cs7 cs8
>   Select character size, if possible. This shall have the effect of setting CS5, CS6, CS7, and CS8, respectively, in the termios c_cflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> number
>   Set terminal baud rate to the number given, if possible. If the baud rate is set to zero, the modem control lines shall no longer be asserted. This shall have the effect of setting the input and output termios baud rate values as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ispeed number
>   Set terminal input baud rate to the number given, if possible. If the input baud rate is set to zero, the input baud rate shall be specified by the value of the output baud rate. This shall have the effect of setting the input termios baud rate values as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ospeed number
>   Set terminal output baud rate to the number given, if possible. If the output baud rate is set to zero, the modem control lines shall no longer be asserted. This shall have the effect of setting the output termios baud rate values as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> hupcl (-hupcl)
>   Stop asserting modem control lines (do not stop asserting modem control lines) on last close. This shall have the effect of setting (not setting) HUPCL in the termios c_cflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> hup (-hup)
>   Equivalent to hupcl( -hupcl).
> cstopb (-cstopb)
>   Use two (one) stop bits per character. This shall have the effect of setting (not setting) CSTOPB in the termios c_cflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> cread (-cread)
>   Enable (disable) the receiver. This shall have the effect of setting (not setting) CREAD in the termios c_cflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> clocal (-clocal)
>   Assume a line without (with) modem control. This shall have the effect of setting (not setting) CLOCAL in the termios c_cflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.

> It is unspecified whether stty shall report an error if an attempt to set a Control Mode fails.

> ##### Input Modes

> ignbrk (-ignbrk)
>   Ignore (do not ignore) break on input. This shall have the effect of setting (not setting) IGNBRK in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> brkint (-brkint)
>   Signal (do not signal) INTR on break. This shall have the effect of setting (not setting) BRKINT in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ignpar (-ignpar)
>   Ignore (do not ignore) bytes with parity errors. This shall have the effect of setting (not setting) IGNPAR in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> parmrk (-parmrk)
>   Mark (do not mark) parity errors. This shall have the effect of setting (not setting) PARMRK in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> inpck (-inpck)
>   Enable (disable) input parity checking. This shall have the effect of setting (not setting) INPCK in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> istrip (-istrip)
>   Strip (do not strip) input characters to seven bits. This shall have the effect of setting (not setting) ISTRIP in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> inlcr (-inlcr)
>   Map (do not map) NL to CR on input. This shall have the effect of setting (not setting) INLCR in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> igncr (-igncr)
>   Ignore (do not ignore) CR on input. This shall have the effect of setting (not setting) IGNCR in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> icrnl (-icrnl)
>   Map (do not map) CR to NL on input. This shall have the effect of setting (not setting) ICRNL in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ixon (-ixon)
>   Enable (disable) START/STOP output control. Output from the system is stopped when the system receives STOP and started when the system receives START. This shall have the effect of setting (not setting) IXON in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ixany (-ixany)
>   [XSI] Allow any character to restart output. This shall have the effect of setting (not setting) IXANY in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ixoff (-ixoff)
>   Request that the system send (not send) STOP characters when the input queue is nearly full and START characters to resume data transmission. This shall have the effect of setting (not setting) IXOFF in the termios c_iflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.

> ##### Output Modes

> opost (-opost)
>   Post-process output (do not post-process output; ignore all other output modes). This shall have the effect of setting (not setting) OPOST in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ocrnl (-ocrnl)
>   [XSI] Map (do not map) CR to NL on output This shall have the effect of setting (not setting) OCRNL in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> onocr (-onocr)
>   Do not (do) output CR at column zero. This shall have the effect of setting (not setting) ONOCR in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> onlret (-onlret)
>   The terminal newline key performs (does not perform) the CR function. This shall have the effect of setting (not setting) ONLRET in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ofill (-ofill)
>   Use fill characters (use timing) for delays. This shall have the effect of setting (not setting) OFILL in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ofdel (-ofdel)
>   Fill characters are DELs (NULs). This shall have the effect of setting (not setting) OFDEL in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> cr0 cr1 cr2 cr3
>   Select the style of delay for CRs. This shall have the effect of setting CRDLY to CR0, CR1, CR2, or CR3, respectively, in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> nl0 nl1
>   Select the style of delay for NL. This shall have the effect of setting NLDLY to NL0 or NL1, respectively, in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> tab0 tab1 tab2 tab3
>   Select the style of delay for horizontal tabs. This shall have the effect of setting TABDLY to TAB0, TAB1, TAB2, or TAB3, respectively, in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface. Note that TAB3 has the effect of expanding <tab>s to <space>s.
> tabs (-tabs)
>   Synonym for tab0 ( tab3).
> bs0 bs1
>   Select the style of delay for backspaces. This shall have the effect of setting BSDLY to BS0 or BS1, respectively, in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> ff0 ff1
>   Select the style of delay for form-feeds. This shall have the effect of setting FFDLY to FF0 or FF1, respectively, in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> vt0 vt1
>   Select the style of delay for vertical-tabs. This shall have the effect of setting VTDLY to VT0 or VT1, respectively, in the termios c_oflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.

> ##### Local Modes

> isig (-isig)
>   Enable (disable) the checking of characters against the special control characters INTR, QUIT, and SUSP. This shall have the effect of setting (not setting) ISIG in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> icanon (-icanon)
>   Enable (disable) canonical input (ERASE and KILL processing). This shall have the effect of setting (not setting) ICANON in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> iexten (-iexten)
>   Enable (disable) any implementation-defined special control characters not currently controlled by icanon, isig, ixon, or ixoff. This shall have the effect of setting (not setting) IEXTEN in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> echo (-echo)
>   Echo back (do not echo back) every character typed. This shall have the effect of setting (not setting) ECHO in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> echoe (-echoe)
>   The ERASE character visually erases (does not erase) the last character in the current line from the display, if possible. This shall have the effect of setting (not setting) ECHOE in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> echok (-echok)
>   Echo (do not echo) NL after KILL character. This shall have the effect of setting (not setting) ECHOK in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> echonl (-echonl)
>   Echo (do not echo) NL, even if echo is disabled. This shall have the effect of setting (not setting) ECHONL in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> noflsh (-noflsh)
>   Disable (enable) flush after INTR, QUIT, SUSP. This shall have the effect of setting (not setting) NOFLSH in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.
> tostop (-tostop)
>   Send SIGTTOU for background output. This shall have the effect of setting (not setting) TOSTOP in the termios c_lflag field, as defined in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface.

> ##### Special Control Character Assignments

> <control>-character string
>   Set <control>-character to string. If <control>-character is one of the character sequences in the first column of the following table, the corresponding Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface control character from the second column shall be recognized. This has the effect of setting the corresponding element of the termios c_cc array (see the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 13, Headers, <termios.h>).
>   Table: Control Character Names in stty

>   Control Character | c_cc Subscript | Description
>   --- | --- | ---
>   eof | VEOF | EOF character
>   eol | VEOL | EOL character
>   erase | VERASE | ERASE character
>   intr | VINTR | INTR character
>   kill | VKILL | KILL character
>   quit | VQUIT | QUIT character
>   susp | VSUSP | SUSP character
>   start | VSTART | START character
>   stop | VSTOP | STOP character

>   If string is a single character, the control character shall be set to that character. If string is the two-character sequence `"^-"` or the string undef, the control character shall be set to _POSIX_VDISABLE , if it is in effect for the device; if _POSIX_VDISABLE is not in effect for the device, it shall be treated as an error. In the POSIX locale, if string is a two-character sequence beginning with circumflex ( `'^'` ), and the second character is one of those listed in the `"^c"` column of the following table, the control character shall be set to the corresponding character value in the Value column of the table.

>   Table: Circumflex Control Characters in stty

>   ^c | Value | ^c | Value | ^c | Value
>   --- | --- | --- | --- | --- | ---
>   a, A | <SOH> | l, L | <FF> | w, W | <ETB> |  |  |  |  |
>   b, B | <STX> | m, M | <CR> | x, X | <CAN> |  |  |  |  |
>   c, C | <ETX> | n, N | <SO> | y, Y | <EM> |  |  |  |  |
>   d, D | <EOT> | o, O | <SI> | z, Z | <SUB> |  |  |  |  |
>   e, E | <ENQ> | p, P | <DLE> | [ | <ESC> |  |  |  |  |
>   f, F | <ACK> | q, Q | <DC1> | \ | <FS> |  |  |  |  |
>   g, G | <BEL> | r, R | <DC2> | ] | <GS> |  |  |  |  |
>   h, H | <BS> | s, S | <DC3> | ^ | <RS> |  |  |  |  |
>   i, I | <HT> | t, T | <DC4> | _ | <US> |  |  |  |  |
>   j, J | <LF> | u, U | <NAK> | ? | <DEL> |  |  |  |  |
>   k, K | <VT> | v, V | <SYN> |  |  |  |  |  |  |

> min number
>   Set the value of MIN to number. MIN is used in non-canonical mode input processing ( icanon).
> time number
>   Set the value of TIME to number. TIME is used in non-canonical mode input processing ( icanon).

> ##### Combination Modes

> saved settings
>   Set the current terminal characteristics to the saved settings produced by the -g option.
> evenp or parity
>   Enable parenb and cs7; disable parodd.
> oddp
>   Enable parenb, cs7, and parodd.
> -parity, -evenp, or -oddp
>   Disable parenb, and set cs8.
> raw (-raw or cooked)
>   [XSI]
>   Enable (disable) raw input and output. Raw mode shall be equivalent to setting:

>       stty cs8 erase ^- kill ^- intr ^- \
>           quit ^- eof ^- eol ^- -post -inpck

> nl (-nl)
>   Disable (enable) icrnl. In addition, -nl unsets inlcr and igncr.
> ek
>   Reset ERASE and KILL characters back to system defaults.
> sane
>   Reset all modes to some reasonable, unspecified, values.

#### STDIN

> Although no input is read from standard input, standard input shall be used to get the current terminal I/O characteristics and to set new terminal I/O characteristics.

#### INPUT FILES

> None.

#### ENVIRONMENT VARIABLES

> The following environment variables shall affect the execution of stty:

> LANG
>   Provide a default value for the internationalization variables that are unset or null. (See the Base Definitions volume of IEEE Std 1003.1-2001, Section 8.2, Internationalization Variables for the precedence of internationalization variables used to determine the values of locale categories.)
> LC_ALL
>   If set to a non-empty string value, override the values of all the other internationalization variables.
> LC_CTYPE
>   This variable determines the locale for the interpretation of sequences of bytes of text data as characters (for example, single-byte as opposed to multi-byte characters in arguments) and which characters are in the class print.
> LC_MESSAGES
>   Determine the locale that should be used to affect the format and contents of diagnostic messages written to standard error.
> NLSPATH
>   [XSI] Determine the location of message catalogs for the processing of LC_MESSAGES .

#### ASYNCHRONOUS EVENTS

> Default.

#### STDOUT

> If operands are specified, no output shall be produced.

> If the -g option is specified, stty shall write to standard output the current settings in a form that can be used as arguments to another instance of stty on the same system.

> If the -a option is specified, all of the information as described in the OPERANDS section shall be written to standard output. Unless otherwise specified, this information shall be written as <space>-separated tokens in an unspecified format, on one or more lines, with an unspecified number of tokens per line. Additional information may be written.

> If no options or operands are specified, an unspecified subset of the information written for the -a option shall be written.

> If speed information is written as part of the default output, or if the -a option is specified and if the terminal input speed and output speed are the same, the speed information shall be written as follows:

>     "speed %d baud;", <speed>

> Otherwise, speeds shall be written as:

>     "ispeed %d baud; ospeed %d baud;", <ispeed>, <ospeed>

> In locales other than the POSIX locale, the word baud may be changed to something more appropriate in those locales.

> If control characters are written as part of the default output, or if the -a option is specified, control characters shall be written as:

>     "%s = %s;", <control-character name>, <value>

> where <value> is either the character, or some visual representation of the character if it is non-printable, or the string undef if the character is disabled.

#### STDERR

> The standard error shall be used only for diagnostic messages.

#### OUTPUT FILES

> None.

#### EXTENDED DESCRIPTION

> None.

#### EXIT STATUS

> The following exit values shall be returned:

> 0
>   The terminal options were read or set successfully.
> >0
>   An error occurred.

#### CONSEQUENCES OF ERRORS

> Default.

The following sections are informative.

#### APPLICATION USAGE

> The -g flag is designed to facilitate the saving and restoring of terminal state from the shell level. For example, a program may:

>     saveterm="$(stty -g)"       # save terminal state
>     stty (new settings)         # set new state
>     ...                         # ...
>     stty $saveterm              # restore terminal state

> Since the format is unspecified, the saved value is not portable across systems.

> Since the -a format is so loosely specified, scripts that save and restore terminal settings should use the -g option.

#### EXAMPLES

> None.

#### RATIONALE

> The original stty description was taken directly from System V and reflected the System V terminal driver termio. It has been modified to correspond to the terminal driver termios.

> Output modes are specified only for XSI-conformant systems. All implementations are expected to provide stty operands corresponding to all of the output modes they support.

> The stty utility is primarily used to tailor the user interface of the terminal, such as selecting the preferred ERASE and KILL characters. As an application programming utility, stty can be used within shell scripts to alter the terminal settings for the duration of the script.

> The termios section states that individual disabling of control characters is possible through the option _POSIX_VDISABLE. If enabled, two conventions currently exist for specifying this: System V uses `"^-"`, and BSD uses undef. Both are accepted by stty in this volume of IEEE Std 1003.1-2001. The other BSD convention of using the letter `'u'` was rejected because it conflicts with the actual letter `'u'`, which is an acceptable value for a control character.

> Early proposals did not specify the mapping of `"^c"` to control characters because the control characters were not specified in the POSIX locale character set description file requirements. The control character set is now specified in the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 3, Definitions so the historical mapping is specified. Note that although the mapping corresponds to control-character key assignments on many terminals that use the ISO/IEC 646:1991 standard (or ASCII) character encodings, the mapping specified here is to the control characters, not their keyboard encodings.

> Since termios supports separate speeds for input and output, two new options were added to specify each distinctly.

> Some historical implementations use standard input to get and set terminal characteristics; others use standard output. Since input from a login TTY is usually restricted to the owner while output to a TTY is frequently open to anyone, using standard input provides fewer chances of accidentally (or maliciously) altering the terminal settings of other users. Using standard input also allows stty -a and stty -g output to be redirected for later use. Therefore, usage of standard input is required by this volume of IEEE Std 1003.1-2001.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> Shell Command Language, the Base Definitions volume of IEEE Std 1003.1-2001, Chapter 11, General Terminal Interface, <termios.h>

#### CHANGE HISTORY

> First released in Issue 2.

#### Issue 5

> The description of tabs is clarified.

> The FUTURE DIRECTIONS section is added.

#### Issue 6

> The legacy items iuclc(- iuclc), xcase, olcuc(- olcuc), lcase(- lcase), and LCASE(- LCASE) are removed.

> IEEE Std 1003.1-2001/Cor 1-2002, item XCU/TC1/D6/37 is applied, applying IEEE PASC Interpretation 1003.2 #133, fixing an error in the OPERANDS section for the Combination Modes nl( -nl).

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]