The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> sys/un.h - definitions for UNIX domain sockets

#### SYNOPSIS

> `#include <sys/un.h>`

#### DESCRIPTION

> The <sys/un.h> header shall define the sockaddr_un structure that includes at least the following members:

>     sa_family_t  sun_family  Address family.
>     char         sun_path[]  Socket pathname.

> The sockaddr_un structure is used to store addresses for UNIX domain sockets. Values of this type shall be cast by applications to struct sockaddr for use with socket functions.

> The sa_family_t type shall be defined as described in <sys/socket.h>.

The following sections are informative.

#### APPLICATION USAGE

> The size of sun_path has intentionally been left undefined. This is because different implementations use different sizes. For example, 4.3 BSD uses a size of 108, and 4.4 BSD uses a size of 104. Since most implementations originate from BSD versions, the size is typically in the range 92 to 108.

> Applications should not assume a particular length for sun_path or assume that it can hold {_POSIX_PATH_MAX} characters (255).

#### RATIONALE

> None.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> <sys/socket.h>, the System Interfaces volume of IEEE Std 1003.1-2001, bind(), socket(), socketpair()

#### CHANGE HISTORY

> First released in Issue 6. Derived from the XNS, Issue 5.2 specification.

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]