The Open Group Base Specifications Issue 6
IEEE Std 1003.1, 2004 Edition
Copyright © 2001-2004 The IEEE and The Open Group, All Rights reserved.

#### NAME

> shmget - get an XSI shared memory segment

#### SYNOPSIS

> ``[XSI] #include <sys/shm.h>
> int shmget(key_t` key`, size_t` size`, int` shmflg`);``
> `
> `

#### DESCRIPTION

> The shmget() function operates on XSI shared memory (see the Base Definitions volume of IEEE Std 1003.1-2001, Section 3.340, Shared Memory Object). It is unspecified whether this function interoperates with the realtime interprocess communication facilities defined in Realtime.

> The shmget() function shall return the shared memory identifier associated with key.

> A shared memory identifier, associated data structure, and shared memory segment of at least size bytes (see <sys/shm.h>) are created for key if one of the following is true:

> - The argument key is equal to IPC_PRIVATE.

> - The argument key does not already have a shared memory identifier associated with it and (shmflg &IPC_CREAT) is non-zero.

> Upon creation, the data structure associated with the new shared memory identifier shall be initialized as follows:

> - The values of shm_perm.cuid, shm_perm.uid, shm_perm.cgid, and shm_perm.gid are set equal to the effective user ID and effective group ID, respectively, of the calling process.

> - The low-order nine bits of shm_perm.mode are set equal to the low-order nine bits of shmflg.

> - The value of shm_segsz is set equal to the value of size.

> - The values of shm_lpid, shm_nattch, shm_atime, and shm_dtime are set equal to 0.

> - The value of shm_ctime is set equal to the current time.

> When the shared memory segment is created, it shall be initialized with all zero values.

#### RETURN VALUE

> Upon successful completion, shmget() shall return a non-negative integer, namely a shared memory identifier; otherwise, it shall return -1 and set errno to indicate the error.

#### ERRORS

> The shmget() function shall fail if:

> [EACCES
>   A shared memory identifier exists for key but operation permission as specified by the low-order nine bits of shmflg would not be granted; see XSI Interprocess Communication.
> [EEXIST]
>   A shared memory identifier exists for the argument key but (shmflg &IPC_CREAT) &&(shmflg &IPC_EXCL) is non-zero.
> [EINVAL]
>   A shared memory segment is to be created and the value of size is less than the system-imposed minimum or greater than the system-imposed maximum.
> [EINVAL]
>   No shared memory segment is to be created and a shared memory segment exists for key but the size of the segment associated with it is less than size and size is not 0.
> [ENOENT]
>   A shared memory identifier does not exist for the argument key and (shmflg &IPC_CREAT) is 0.
> [ENOMEM]
>   A shared memory identifier and associated shared memory segment shall be created, but the amount of available physical memory is not sufficient to fill the request.
> [ENOSPC]
>   A shared memory identifier is to be created, but the system-imposed limit on the maximum number of allowed shared memory identifiers system-wide would be exceeded.

The following sections are informative.

#### EXAMPLES

> None.

#### APPLICATION USAGE

> The POSIX Realtime Extension defines alternative interfaces for interprocess communication. Application developers who need to use IPC should design their applications so that modules using the IPC routines described in XSI Interprocess Communication can be easily modified to use the alternative interfaces.

#### RATIONALE

> None.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> XSI Interprocess Communication, Realtime, shmat(), shmctl(), shmdt(), shm_open(), shm_unlink(), the Base Definitions volume of IEEE Std 1003.1-2001, <sys/shm.h>

#### CHANGE HISTORY

> First released in Issue 2. Derived from Issue 2 of the SVID.

#### Issue 5

> Moved from SHARED MEMORY to BASE.

> The note about use of POSIX Realtime Extension IPC routines has been moved from FUTURE DIRECTIONS to a new APPLICATION USAGE section.

End of informative text.

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
[ Main Index | XBD | XCU | XSH | XRAT ]